**My MAC Address:**

90:E8:68:2C:7F:43

**My IP Address:**

10.116.31.185

**Pinging my neighbors IP Address:**



**Request:**

Frame 15575: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface \Device\NPF\_{2FB47E7F-2722-4432-BF1C-D1639583CA2B}, id 0

Ethernet II, Src: AzureWav\_2c:7f:43 (90:e8:68:2c:7f:43), Dst: IntelCor\_04:58:00 (6c:a1:00:04:58:00)

Address Resolution Protocol (request)

Hardware type: Ethernet (1)

Protocol type: IPv4 (0x0800)

Hardware size: 6

Protocol size: 4

Opcode: request (1)

Sender MAC address: AzureWav\_2c:7f:43 (90:e8:68:2c:7f:43)

Sender IP address: 10.116.31.185

Target MAC address: IntelCor\_04:58:00 (6c:a1:00:04:58:00)

Target IP address: 10.116.30.9

**Response:**

Frame 15577: 56 bytes on wire (448 bits), 56 bytes captured (448 bits) on interface \Device\NPF\_{2FB47E7F-2722-4432-BF1C-D1639583CA2B}, id 0

Ethernet II, Src: IntelCor\_04:58:00 (6c:a1:00:04:58:00), Dst: AzureWav\_2c:7f:43 (90:e8:68:2c:7f:43)

Address Resolution Protocol (reply)

Hardware type: Ethernet (1)

Protocol type: IPv4 (0x0800)

Hardware size: 6

Protocol size: 4

Opcode: reply (2)

Sender MAC address: IntelCor\_04:58:00 (6c:a1:00:04:58:00)

Sender IP address: 10.116.30.9

Target MAC address: AzureWav\_2c:7f:43 (90:e8:68:2c:7f:43)

Target IP address: 10.116.31.185